{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["min_reb","Sheet2","Sheet2 (2)"],"not_rendered":{"charts":8,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"min_reb","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[]}
[null,null,null,null,"The ratio increases with velocity, but a general rule of thumb is that comp should be stiffer than reb at low velocities.."]
[null,null,null,null,"The ratio varies from less than 1 at low velocities to slightly more than 2 at higher velocities."]
[" 5-6-24",null,null,null,"Using rule of thumb that reb should  be lighter than comp at low velocities."]
["We created  dynoshock_press ",null,null,null,"We can assume there is a min amount of reb needed depending on the application.  And there is a bare minimum needed for any application."]
["TABLE and are redoing the"]
["comments on  'minimum reb"]
["force needed for any",null,null,null,"Depending on the application, we can assume there is a min amount of reb and comp force needed"]
["application'.",null,null,null,"The reb comp ratio [r/c ratio] shows a relationship between reb and comp forces at specific velocities."]
[null,null,null,null,"The ratio increases with velocity, but a general rule of thumb is that reb should be faster than comp at low velocities."]
[" a_open_press_linear.php",null,null,null,"For example:   55 lbs reb force,  69 lbs comp force  (55 / 69 = .80)"]
[]
[null,null,null,null,"r/c ratio less than 1 . . . comp is stiffer"]
[null,null,null,null,"min reb",45,50,55,60,65]
[null,null,null,null,"comp",{"$f":"F13/F15","v":50},{"$f":"G13/G15","v":55.555555555555557},{"$f":"H13/H15","v":61.111111111111107},{"$f":"I13/I15","v":66.666666666666671},{"$f":"J13/J15","v":72.222222222222214}]
[null,null,null,null," r/c ratio",0.9,0.9,0.9,0.9,0.9]
[]
[null,null,null,null,"min reb",45,50,55,60,65]
[null,null,null,null,"comp",{"$f":"F17/F19","v":56.25},{"$f":"G17/G19","v":62.5},{"$f":"H17/H19","v":68.75},{"$f":"I17/I19","v":75},{"$f":"J17/J19","v":81.25}]
[null,null,null,null," r/c ratio",0.8,0.8,0.8,0.8,0.8]
[]
[null,null,null,null,"min reb",45,50,55,60,65]
[null,null,null,null,"comp",{"$f":"F21/F23","v":64.285714285714292},{"$f":"G21/G23","v":71.428571428571431},78.571428571428569,85.714285714285722,92.857142857142861]
[null,null,null,null," r/c ratio",0.7,0.7,0.7,0.7,0.7]

{"sheet":"Sheet2","index":1,"n_rows":63,"n_cols":7,"rows_kept":63,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,null,null,"ips","ro wogas","co wogas","r/c ratio"]
[null,null,null,null,"[actual]","[actual]","[actual]"]
[null,null,null,1]
[null,null,null,2,-55.7,74.099999999999994,0.75]
[null,null,null,3,-75.2,95,0.79]
[null,null,null,4,-97.3,112.2,0.87]
[null,null,null,5,-121.4,128.4,0.95]
[null,null,null,10,-245.8,204,1.21]
[null,null,null,20,-494.2,345.4,1.43]
[null,null,null,30,-739.9,467.3,1.58]
[null,null,null,40,-999,580.29999999999995,1.72]
[null,null,null,50,-1253.2,683.4,1.83]
[]
[]
[]
[null,null,null,"ips","ro wogas","co wogas","r/c ratio"]
[null,null,null,null,"[linear]","[linear]","[linear]"]
[null,null,null,1]
[null,null,null,2,-55.7,74.099999999999994,0.75]
[null,null,null,3,-80.599999999999994,87.2,0.93]
[null,null,null,4,-105.6,97.9,1.08]
[null,null,null,5,-130.5,110.3,1.18]
[null,null,null,10,-255.3,174.4,1.46]
[null,null,null,20,-504.8,302.39999999999998,1.67]
[null,null,null,30,-754.2,428.2,1.76]
[null,null,null,40,-1003.7,556.20000000000005,1.8]
[null,null,null,50,-1253.2,683.3,1.83]
[]
[]
[]
[null,null,null,"ips","ro wogas","ro wogas","lb diff"]
[null,null,null,null,"[actual]","[linear]","[1-2]"]
[null,{"$f":"-E35","v":-35.1},null,1,35.1]
[null,{"$f":"-E36","v":-55.7},-55.7,2,55.7,55.7,0]
[null,-75.2,-80.599999999999994,3,75.2,80.599999999999994,-5.4]
[null,-97.3,-105.6,4,97.3,105.6,-8.3000000000000007]
[null,-121.4,-130.5,5,121.4,130.5,-9.1999999999999993]
[null,-245.8,-255.3,10,245.8,255.3,-9.5]
[null,-494.2,-504.8,20,494.2,504.8,-10.5]
[null,-739.9,-754.2,30,739.9,754.2,-14.4]
[null,-999,-1003.7,40,999,1003.7,-4.7]
[null,-1253.2,-1253.2,50,1253.2,1253.2,0]
[]
[]
[]
[null,null,null,"ips","ro wogas","ro wogas","lb diff"]
[null,null,null,null,"[actual]","[linear]","[1-2]"]
[null,null,null,1,35.1]
[null,null,null,2,55.7,55.7,0]
[null,null,null,3,75.2,80.599999999999994,-5.4]
[null,null,null,4,97.3,105.6,-8.3000000000000007]
[null,null,null,5,121.4,130.5,-9.1999999999999993]
[null,null,null,6,{"$f":"intrp(D55,D36:D44,E36:E44)","v":146.28}]
[null,null,null,7,{"$f":"intrp(D56,D37:D45,E37:E45)","v":175.44800000000009}]
[null,null,null,8,{"$f":"intrp(D57,D38:D46,E38:E46)","v":200.51199999999994}]
[null,null,null,9,{"$f":"intrp(D58,D39:D47,E39:E47)","v":225.57600000000002}]
[null,null,null,10,245.8,255.3,-9.5]
[null,null,null,20,494.2,504.8,-10.5]
[null,null,null,30,739.9,754.2,-14.4]
[null,null,null,40,999,1003.7,-4.7]
[null,null,null,50,1253.2,1253.2,0]

{"sheet":"Sheet2 (2)","index":2,"n_rows":63,"n_cols":10,"rows_kept":63,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,null,null,"ips","ro wogas","co wogas","r/c ratio"]
[null,null,null,null,"[actual]","[actual]","[actual]"]
[null,null,null,1]
[null,null,null,2,-55.7,74.099999999999994,0.75]
[null,null,null,3,-75.2,95,0.79]
[null,null,null,4,-97.3,112.2,0.87]
[null,null,null,5,-121.4,128.4,0.95]
[null,null,null,10,-245.8,204,1.21]
[null,null,null,20,-494.2,345.4,1.43]
[null,null,null,30,-739.9,467.3,1.58]
[null,null,null,40,-999,580.29999999999995,1.72]
[null,null,null,50,-1253.2,683.4,1.83]
[]
[]
[]
[null,null,null,"ips","ro wogas","co wogas","r/c ratio"]
[null,null,null,null,"[linear]","[linear]","[linear]"]
[null,null,null,1]
[null,null,null,2,-55.7,74.099999999999994,0.75]
[null,null,null,3,-80.599999999999994,87.2,0.93]
[null,null,null,4,-105.6,97.9,1.08]
[null,null,null,5,-130.5,110.3,1.18]
[null,null,null,10,-255.3,174.4,1.46]
[null,null,null,20,-504.8,302.39999999999998,1.67]
[null,null,null,30,-754.2,428.2,1.76]
[null,null,null,40,-1003.7,556.20000000000005,1.8]
[null,null,null,50,-1253.2,683.3,1.83]
[]
[]
[]
[null,null,null,"ips","c force","c force","lb diff"]
[null,null,null,null,"[actual]","[linear]","[1-2]"]
[null,{"$f":"-E35","v":-31},null,1,31]
[null,{"$f":"-E36","v":-64.900000000000006},-64.900000000000006,2,64.900000000000006,64.900000000000006,0,{"$f":"E36/F36","v":1}]
[null,-84.5,-75.8,3,84.5,75.8,8.6999999999999993,{"$f":"E37/F37","v":1.1147757255936677}]
[null,-102.3,-86.7,4,102.3,86.7,15.5,1.1799307958477507]
[null,-117.4,-97.6,5,117.4,97.6,19.7,1.2028688524590165]
[null,-181.2,-152.1,10,181.2,152.1,29.1,1.1913214990138066,null,{"$f":"152*1.2","v":182.4}]
[null,-295.10000000000002,-261.2,20,295.10000000000002,261.2,33.9,1.1297856049004595]
[null,-400.5,-370.2,30,400.5,370.2,30.3,1.0818476499189627]
[null,-498.3,-479.3,40,498.3,479.3,19,1.0396411433340287]
[null,-588.29999999999995,-588.29999999999995,50,588.29999999999995,588.29999999999995,0,1]
[]
[]
[]
[null,null,null,"ips","ro wogas","ro wogas","lb diff"]
[null,null,null,null,"[actual]","[linear]","[1-2]"]
[null,null,null,1,31]
[null,null,null,2,64.900000000000006,64.900000000000006,0]
[null,null,null,3,84.5,75.8,8.6999999999999993]
[null,null,null,4,102.3,86.7,15.5]
[null,null,null,5,117.4,97.6,19.7]
[null,null,null,6,{"$f":"intrp($D55,$D$36:$D$40,E$36:E$40)","v":130.16},{"$f":"intrp($D55,$D$36:$D$40,F$36:F$40)","v":108.5},{"$f":"E55-F55","v":21.659999999999997}]
[null,null,null,7,{"$f":"intrp($D56,$D$36:$D$40,E$36:E$40)","v":142.91999999999999},{"$f":"intrp($D56,$D$36:$D$40,F$36:F$40)","v":119.39999999999999},{"$f":"E56-F56","v":23.519999999999996}]
[null,null,null,8,{"$f":"intrp($D57,$D$36:$D$40,E$36:E$40)","v":155.68},{"$f":"intrp($D57,$D$36:$D$40,F$36:F$40)","v":130.30000000000001},25.379999999999995]
[null,null,null,9,{"$f":"intrp($D58,$D$36:$D$40,E$36:E$40)","v":168.44},{"$f":"intrp($D58,$D$36:$D$40,F$36:F$40)","v":141.19999999999999},27.240000000000009]
[null,null,null,10,181.2,152.1,29.1]
[null,null,null,20,295.10000000000002,261.2,33.9]
[null,null,null,30,400.5,370.2,30.3]
[null,null,null,40,498.3,479.3,19]
[null,null,null,50,588.29999999999995,588.29999999999995,0]